For 1990-2009 cars

Name | 6T40/6T45
--- | ---
RPO Codes | MH8, MH7
Production Location | Korea/China
Transmission Drive | Front Wheel Drive
Reverse Gear Ratio | 2.94
1st Gear Ratio | 4.584
2nd Gear Ratio | 2.964
3rd Gear Ratio | 1.912
4th Gear Ratio | 1.446
5th Gear Ratio | 1.000
6th Gear Ratio | 0.746
Effective Final Drive Gear Ratio | Gasoline Engine: 2.89
Diesel Engine: 2.64
Torque Converter Size - Diameter of Torque Converter Turbine | 236 mm
Pressure Taps Line | Pressure
Transmission Fluid Type | DEXRON VI®
Transmission Fluid Capacity | Gasoline Engine: 8.16 ± 0.12L
Diesel Engine: 8.66 ± 0.12L
Transmission Type: 6 | Six Forward Gears
Transmission Type: T | Transverse Mount
Transmission Type: 40/45 | Product Series
Position Quadrant | P, R, N, D, * *(Refer to the applicable owner's manual)
Case Material | Die Cast Aluminum
Transmission Net Weight | 81/85 kg
Maximum Trailer Towing Capacity | N/A
Maximum Gross Vehicle Weight (GVW) | 4,000 lbs