For 1990-2009 cars

### Removal Procedure

1. Lower the rear seat backs.
2. Remove the retaining clips and reposition the rear seat back cover.
3. Remove the nuts and the armrest.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the armrest with the nuts.

Tighten
Tighten the armrest nuts to 24 N·m (18 lb ft).

2. Install the rear seat back backside cover with the retaining clips.
3. Raise and secure the rear seat backs in the upright position.