For 1990-2009 cars

As the vehicle speed increases, the transmission control module (TCM) receives input signals from the automatic transmission input and output speed sensors, the throttle position sensor and other vehicle sensors to determine the precise moment to command OFF the normally-low 26 pressure control solenoid 4. At the same time the 35R pressure control solenoid 2 is also commanded ON to regulate 3-5 clutch apply.

### 3-5 Reverse Clutch Applies

#### 35R Pressure Control Solenoid 2

The 35R pressure control solenoid 2 is commanded ON allowing actuator feed fluid to enter the pressure control solenoid (PCS) 35 reverse clutch fluid circuit. PCS 35 reverse clutch fluid is routed through orifice #26 and then to the 3-5 reverse clutch regulator valve. PCS 35 reverse clutch fluid is also routed through to the 1-2-3-4 clutch boost valve, but is blocked by the spacer plate gasket from entering the PCS 1234 clutch circuit.

#### 3-5 Reverse Clutch Regulator Valve

PCS 35 reverse clutch fluid moves the 3-5 reverse clutch regulator valve against 3-5 reverse clutch regulator valve spring force and 35 reverse clutch feedback fluid. This allows 35 reverse feed to pass through the valve and enter the 35 reverse clutch circuit. The 35 reverse clutch fluid is then routed to the 3-5 reverse clutch, through orifice #6 to the spring area of the 35 reverse clutch regulator valve and through orifice #33 to ball check valve 6. When the 3-5 reverse clutch regulator valve is in this position, PS2 fluid from the pressure switch 2 exhausts through the valve allowing the switch to close.

#### 3-5 Reverse Clutch

The 35 reverse clutch fluid enters the 3-5 reverse/4-5-6 clutch housing to move the piston against spring force to apply the 3-5 reverse clutch plates.

### 2-6 Clutch Releases

#### 26 Pressure Control Solenoid 4

The 26 pressure control solenoid 4 is commanded OFF allowing PCS 26 clutch fluid from the 2-6 clutch regulator valve to exhaust. The drive fluid at the 2-6 clutch regulator valve passes through the valve and enters the PS3 fluid circuit. PS3 fluid is then routed to pressure switch 2 and opens the normally-closed switch.

#### 2-6 Clutch Regulator Valve

The 2-6 clutch regulator valve spring force moves the valve to allow 26 clutch fluid from the 2-6 clutch to pass through the valve and enter the exhaust backfill fluid circuit.

#### 2-6 Clutch

The 2-6 clutch spring force moves the 2-6 clutch piston to release the 2-6 clutch plates and forces 26 clutch fluid to exhaust. The 26 clutch fluid is routed through the 2-6 clutch regulator valve where it enters the exhaust backfill fluid circuit and is exhausted.

#### Drive Range, Third Gear