For 1990-2009 cars

1. Install the forward clutch and direct clutch assembly (23). Rotate the clutch assembly during installation in order to index the forward and direct clutch plates with the rear internal gear and the rear sun gear assembly.
2. Measure dimension a.

Installation Height
Dimension a should be 50.850-51.825 mm (2.002-2.040 in).

3. If dimension a is greater than specification, index the forward and direct clutch assembly until the correct specification is met.

Note: Do not bend or damage the lube fluid pipe.

4. Using a plastic hammer, install the lube fluid pipe (85).
5. Install the lube fluid pipe retainer (84)

Caution: Refer to Fastener Caution in the Preface section.

6. Install the lube fluid pipe retainer bolt (83) and tighten to 5 N·m (44 lb in)..
7. Apply grease to the 5 new case fluid passage seals.
8. Install the 5 new case fluid passage seals (86) into the transmission case assembly.