For 1990-2009 cars

### Removal Procedure

1. Remove the clip on the vacuum hose connection at the intake manifold.
2. Remove the hose from the union nut connection.
3. Remove the clip on the vacuum hose connection to the brake booster.
4. Remove the vacuum hose.

### Installation Procedure

1. Mount the vacuum hose and ensure the connections are tight on each end.
2. Install the vacuum hose clips.