For 1990-2009 cars

1. Install the 2 third gear band apply tube O-ring seals (53).
2. Install the third gear band apply tube (52).
3. If needed, lightly seat the third gear band apply tube into the transmission case assembly with a soft mallet.
4. Install the third gear band apply tube retainer (51).

Caution: Refer to Fastener Caution in the Preface section.

5. Install the 2 - M6 x 1.0 x 14 mm third gear band apply tube retainer bolts (50) and tighten to 5 N·m (44 lb in).