For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Low and Reverse Clutch Assembly (OWC) Tip

• | The Low and Reverse Clutch Assembly should rotate freely in one direction and lock in the opposite direction.

• | Align the large flat areas of the Low and Reverse Clutch Assembly with the valve body end of the case.

2 | Low and Reverse Clutch Backing Plate
3 | Low and Reverse Clutch Plate Assembly (Qty: 3)
4 | Low and Reverse Clutch Plate (Qty: 3) Tip Align the large flat areas of the Low and Reverse Clutch Plate with the valve body end of the case.
5 | Low and Reverse Clutch Apply (Waved) Plate Tip Align the large flat areas of the Low and Reverse Clutch Apply Plate with the valve body end of the case.