For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the rear wheels.
3. Remove the upper arm nut-to-rear knuckle.
4. Remove the nuts upper arm-to-body.
5. Remove the upper arm.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the upper arm with nuts-to-body.

Tighten
Tighten the upper arm nuts-to-body to 60 N·m (44 lb ft).

2. Install the upper arm nut-to-rear knuckle.

Tighten
Tighten the upper arm nut-to-rear knuckle to 110 N·m (81 lb ft).