For 1990-2009 cars

### Removal Procedure

1. Remove the front door escutcheon.
2. Disconnect the mirror electrical connector if the mirror is electronically controlled.
3. Remove the bolts and the outside rearview mirror assembly from the door.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the outside rearview mirror assembly to the door with the screws.

Tighten
Tighten the outside rearview mirror assembly screws to 4.5 N·m (40 lb in).

2. Connect the mirror electrical connector if the mirror is electronically controlled.
3. Install the front door escutcheon.