For 1990-2009 cars

### Removal Procedure

Caution: Refer to Vehicle Lifting and Jacking Caution in the Preface section.

1. Raise and suitably support the vehicle.
2. Remove the front wheel. Refer to Tire and Wheel Removal and Installation.
3. Remove the front mud guard. Refer to Rear Mud Flap Guard Replacement.
4. Remove the screws and the front wheel well splash shield.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the screws and the front wheel well splash shield. Tighten the front wheel well splash shield screws to 2 N·m (18 lb in).
2. Install the front mud guard. Refer to Rear Mud Flap Guard Replacement.
3. Install the front wheel. Refer to Tire and Wheel Removal and Installation.
4. Lower the vehicle.