For 1990-2009 cars

Important: In this adjustment, the right and the left tie rods must be equal in length, or the tires will wear unevenly.

1. Disconnect the outer tie rods from the knuckle assemblies. Refer to Rack and Pinion Outer Tie Rod End Replacement .
2. Loosen the front toe adjusting nut.
3. Turn the right and the left outer tie rods to align the toe to the proper specifications. Refer to Wheel Alignment Specifications .

Notice: Refer to Fastener Notice in the Preface section.

4. Hold the outer tie rod and tighten the front toe adjusting nut.

Tighten
Tighten the front toe adjusting nut to 64 N·m (47 lb ft).

5. Reconnect the outer tie rods to the knuckle assemblies. Refer to Rack and Pinion Outer Tie Rod End Replacement .