For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the air filter outlet hose.
3. Disconnect the crankshaft position (CKP) sensor wiring harness connector.
4. Remove the CKP sensor heat shield housing.
5. Remove the CKP sensor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the CKP sensor.

Tighten
Tighten the CKP sensor retaining bolt to 7 N·m (62 lb in).

2. Install the CKP sensor heat shield housing.

Tighten
Tighten the CKP sensor heat shield housing bolt to 8 N·m (71 lb in).

3. Connect the CKP sensor wiring harness connector.
4. Install the air filter outlet hose.
5. Connect the negative battery cable.