For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear wheels.
3. Remove the upper arm nut-to-rear knuckle.
4. Remove the nuts upper arm-to-body.
5. Remove the upper arm.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the upper arm with nuts-to-body and tighten to 60 N·m (44 lb ft).
2. Install the upper arm nut-to-rear knuckle and tighten to 110 N·m (81 lb ft).