For 1990-2009 cars

#### Transmission Overheats

Condition | Action
--- | ---
DEFINITION: Transmission overheats
Low fluid level | Inspect for leaks and repair as necessary.
Incorrect fluid | Replace the fluid with the correct fluid.
Fluid Filter (42) is restricted |

• | Diagnose the cause for the filter restriction and repair as needed.

• | Replace the fluid filter (42) and fluid.

Restricted Oil Cooler Lines |

• | Inspect for bent or kinked pipes.

• | Inspect for pinched or kinked hoses.

• | Inspect for cracks or signs of hose overheating that may cause delamination of the hose.

• | Replace faulty oil cooler lines.

Internal oil cooler restriction | Replace radiator assembly and fluid.
Case Assembly oil inlet filter/screen |

• | Remove the inlet cooler line seal from the case assembly.

• | Inspect for foreign material trapped by the case inlet filter/screen.

• | Clean the passage to remove the foreign material from the case inlet screen.

| If unable to remove the foreign material, the screen will have to be removed from the case assembly and cleared manually outside of the case assembly.