For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the side marker lamp from the bumper fascia.
3. Remove the bulb from the side marker lamp.

### Installation Procedure

1. Install the bulb into the side marker lamp.
2. Install the side marker lamp into the bumper fascia.
3. Connect the negative battery cable.