For 1990-2009 cars

### Removal Procedure

Important: Left-Hand drive Shown, Right-Hand Drive Similar.

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the screws and the left side portion of the air inlet grille.
3. Remove the nut and the washer that secure the wiper arm linkage to the motor driveshaft.
4. Pry the wiper arm linkage off the motor driveshaft.
5. Disconnect the electrical connector.
6. Remove the bolts and the wiper motor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the wiper motor with the bolts.

Tighten
Tighten the wiper motor bolts to 10 N·m (89 lb in).

2. Connect the electrical connector.
3. Press the wiper arm linkage onto the motor driveshaft.
4. Install the wiper arm linkage to the motor driveshaft with the washer and the nut.

Tighten
Tighten the wiper arm linkage nut to 8.5 N·m (75 lb in).

5. Install the left side portion of the air inlet grille with the screws.

Tighten
Tighten the air inlet grille screws to 2.5 N·m (22 lb in).

6. Connect the negative battery cable.