For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the air filter housing.
3. Remove the output speed sensor electrical connector (4) from the output speed sensor.
4. Remove the output speed sensor bolt.
5. Remove the output speed sensor from the transaxle.
6. Remove the output speed sensor O-ring. Discard the O-ring.

### Installation Procedure

1. Apply the transaxle fluid to the new output speed sensor O-ring.
2. Install the new output speed sensor O-ring onto the input speed sensor.
3. Install the output speed sensor to the transaxle.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the output speed sensor bolt and tighten to 6 N·m (53 lb in).
5. Connect the electrical connector (4) to the output speed sensor.
6. Install the air filter housing.
7. Connect the negative battery cable.