For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the engine under cover.
3. Remove the oil pan drain plug and drain the engine oil.
4. Remove the oil pan flange-to-transaxle bolts.
5. Remove the front engine mount bracket-to-damper bush bolt.
6. Remove the center front suspension member bolts.
7. Remove the oil pan retaining bolts and the oil pan.

### Installation Procedure

Warning: Refer to Eye Protection Warning in the Preface section.

1. Clean the remaining gasket material and oil from the oil pan.
2. Apply new liquid gasket Loctite® 5900-M8585 on the oil pan.
3. Clean any gasket material and oil on the engine mounting surface.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the oil pan and bolts. Tighten the oil pan retaining bolts to 10 N·m (89 lb in).
5. Install the center front suspension member and bolts. Tighten the center front suspension member bolts to 90 N·m (66 lb ft).
6. Install the front engine mount bracket-to-damper bush bolt and tighten to 80 N·m (59 lb ft).
7. Install the oil pan flange-to-transaxle bolts and tighten to 31 N·m (23 lb ft).
8. Discard the used oil pan drain plug washer and replace it with a new one.
9. Discard the used oil pan drain plug washer and replace it with a new one.
10. Install the oil pan drain plug and tighten to 40 N·m (30 lb ft).
11. Refill the engine with engine oil.
12. Install the engine under cover and tighten the retaining bolts to 23 N·m (17 lb ft).
13. Connect the negative battery cable.