For 1990-2009 cars

### Removal Procedure

1. Remove the door seal trim. Refer to Door Bottom Auxiliary Sealing Strip Replacement .
2. Disconnect the outside door handle and the lock rods.
3. Remove the bolts and the door handle.

### Installation Procedure

1. Connect the outside door handle and the lock rods.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the door handle with the bolts.

Tighten
Tighten the outside door handle bolts to 4.5 N·m (40 lb in).

3. Install the door seal trim. Refer to Door Bottom Auxiliary Sealing Strip Replacement .