For 1990-2009 cars

### Removal Procedure

1. Remove the control solenoid valve body and transmission control module (TCM) assembly. Refer to Control Solenoid Valve and Transmission Control Module Assembly Installation.
2. Remove the control solenoid valve support (9).
3. Remove the fluid level control valve gasket (2) and valve (1).
4. Remove the control valve body bolts (3) M6 x 60.
5. Remove the control valve body bolts (4) M6 x 53.
6. Remove the control valve body assembly (5).
7. Remove the control valve body spacer plate assembly (6).

Note: The clutch fluid passage seal is not reusable.

8. Remove the 1-2-3-4 clutch fluid passage seal (7) and low/reverse clutch fluid passage seal (8).

### Installation Procedure

Note: The clutch fluid passage seal is not reusable.

1. Install a NEW 1-2-3-4 clutch fluid passage seal (1) and a NEW low/reverse clutch fluid passage seal (2).
2. Install the control valve body spacer plate assembly (3) to the valve body assembly.

Note: Align the manual valve (a) to the detent lever assembly while installing the control valve body assembly.

3. Install the control valve body assembly (4).

Caution: Refer to Fastener Caution in the Preface section.

Note: Install all bolts before tightening, then tighten in the specified sequence.

4. Install the control valve body bolts (5) M6 x 60 and tighten to 12 N·m (106 lb in).
5. Install the control valve body bolts (6) M6 x 53 and tighten to 12 N·m (106 lb in).
6. Install the fluid level control valve gasket (7) and valve (8).
7. Install the control solenoid valve support (9).
8. Install the control solenoid valve body and transmission control module (TCM) assembly. Refer to Control Solenoid Valve and Transmission Control Module Assembly Installation.