For 1990-2009 cars

### Removal Procedure

Caution: Refer to Sensing and Diagnostic Module Handling Caution in the Preface section.

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disable the SIR system. Refer to SIR Disabling and Enabling
2. Remove the instrument panel (I/P) storage compartment. Refer to Instrument Panel Storage Compartment Replacement .
3. Disconnect the passenger air bag yellow electrical connector.
4. Remove the I/P module by removing the mounting nuts from the upper I/P.

### Installation Procedure

1. Install the I/P module.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the passenger air bag mounting nuts.

Tighten
Tighten the passenger air bag mounting bolts to 7 N·m (62 lb in).

3. Connect the passenger air bag yellow electrical connector.
4. Install the I/P storage compartment. Refer to Instrument Panel Storage Compartment Replacement .
5. Enable the SIR system. Refer to SIR Disabling and Enabling .