For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the rear compartment lamp.
3. Disconnect the electrical connector.
4. Remove the bulb.

### Installation Procedure

1. Install the replacement bulb.
2. Connect the electrical connector.
3. Install the rear compartment lamp.
4. Connect the negative battery cable.