For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the plastic caps and the bolts securing the rear portion of the front seat to the floor.
3. Remove the plastic caps and the bolts securing the front portion of the front seat to the floor.
4. Disconnect the electrical connectors.
5. Remove the seat.

### Installation Procedure

1. Install the seat.
2. Connect the electrical connectors.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the bolts into the front portion of the front seat.

Tighten
Tighten the front seat-to-floor bolts to 25 N·m (18 lb ft).

4. Install the plastic caps.
5. Install the bolts into the rear potion of the front seat.

Tighten
Tighten the front seat-to-floor bolts to 25 N·m (18 lb ft).

6. Install the plastic caps.
7. Connect the negative battery cable.