For 1990-2009 cars

### Removal Procedure

1. Remove the rear molding (1) bonded by the two sided tape.
2. Remove the upper screws.
3. Remove the rear side screws.
4. Remove the retaining clips and the lower screws.
5. Remove the nuts.
6. Remove the rear lower fascia extension.

### Installation Procedure

1. Install the lower fascia extension.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the nuts.

Tighten
Tighten the nuts to 2 N·m (18 lb in).

3. Install the lower screws and clips.

Tighten
Tighten the lower screws to 2 N·m (18 lb in).

4. Install the side screws.

Tighten
Tighten the side screws to 2 N·m (18 lb in).

5. Install the center screws.

Tighten
Tighten the center screws to 2 N·m (18 lb in).

6. Install new two sided tape to the rear molding and install the rear molding (1) to the rear lower fascia extension.