For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the tweeter speaker by prying the tweeter speaker out of the instrument panel.
3. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Install the tweeter speaker into the instrument panel.
3. Connect the negative battery cable.