For 1990-2009 cars

## Front Pipe Replacement Gasoline Engines

### Removal Procedure

Warning: Refer to Exhaust Service Warning in the Preface section.

1. Remove the exhaust lower bracket bolts.
2. Remove the exhaust lower bracket.
3. Remove the exhaust front pipe nuts and the gasket.
4. Remove the nuts that attach the exhaust front pipe to the exhaust front muffler.
5. Remove the gasket from the muffler.
6. Disconnect the exhaust front pipe from the rubber hanger.
7. Remove the exhaust front pipe.
8. Clean the sealing surfaces on the front muffler pipe flange and the exhaust front pipe.
9. Inspect the exhaust front pipe for holes, damage, open seams, or other deterioration which could permit exhaust fumes to seep into the passenger compartment.

### Installation Procedure

1. Install the exhaust front pipe and the gasket.
2. Connect the exhaust front pipe to the rubber hanger.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the exhaust front muffler to the exhaust front pipe and tighten to 30 N·m (22 lb ft).
4. Install the gasket and the exhaust front pipe nuts and tighten to 40 N·m (30 lb ft).
5. Install the exhaust lower bracket.
6. Install the exhaust lower bracket bolts and tighten to 40 N·m (30 lb ft).

## Front Pipe Replacement Diesel Engine

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

Warning: In order to avoid being burned, do not service the exhaust system while it is still hot. Service the system when it is cool.

Caution: When inspecting or replacing exhaust system components, make sure there is adequate clearance from all points on the underbody to prevent overheating of the floor pan and possible damage to the passenger compartment insulation and trim materials.

1. Disconnect the negative battery cable.
2. Disconnect the exhaust gas temperature sensor 1 connector.
3. Remove the rubber hanger.
4. Remove the exhaust front pipe with the gasket. If damaged, replace the new gasket.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the exhaust front pipe and tighten to 40 N·m (29.5 lb ft).
2. Install the rubber hanger.
3. Connect the exhaust gas temperature sensor/connector.
4. Connect the negative battery cables.