For 1990-2009 cars

Danger: To avoid any vehicle damage, serious personal injury or death when major components are removed from the vehicle and the vehicle is supported by a hoist, support the vehicle with jack stands at the opposite end from which the components are being removed and strap the vehicle to the hoist.

Caution: Refer to Vehicle Lifting and Jacking Caution in the Preface section.

Note: On vehicles equipped with rocker panel moldings, the rocker panel molding lower covers MUST be removed prior to lifting.

#### Lifting Points

(1) | Frame Contact Hoist, Lower Rocker Panel Molding Covers
(1) | Frame Contact Hoist, Lower Rocker Panel Molding Covers
(1) | Frame Contact Hoist, Lower Rocker Panel Molding Covers
(1) | Frame Contact Hoist, Lower Rocker Panel Molding Covers
(2) | Floor Jack
(2) | Floor Jack
(2) | Floor Jack
(3) | Suspension Contact Hoist
(3) | Suspension Contact Hoist
(3) | Suspension Contact Hoist
(4) | Center Rocker Lift Point (Left Hand/Right Hand)
(5) | Rear Suspension Axle Lift Point

#### Hoist Locations

(1) | Frame Contact Hoist - Rearward of Front Tire
(2) | Suspension Contact Hoist - Under Front Lower Control Arm
(3) | Suspension Contact Hoist - Lifting on Rear Axle
(4) | Frame Contact Hoist Points for Vehicles Equipped with Lower Rocker Panel Moldings (Covers Removed), Rearward of Front Tires and Forward of Rear Tires
(5) | Frame Contact Hoist - Forward of Rear Tire