For 1990-2009 cars

## Engine Mount Replacement Right Side

#### Tools Required

J 28467-B , DW-117 (DW 110-060) Universal Engine Support Fixture

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

Notice: Refer to Engine Mounting Notice in the Preface section.

1. Disconnect the negative battery cable.

Notice: When raising or supporting the engine for any reason, do not use a jack under the oil pan, any sheet metal, or crankshaft balancer. Jacking against the oil pan may cause it to crack or break.

2. Support the engine assembly using the J 28467-B .
3. Remove the engine mount bracket-to-hydro mount nut and engine mount bracket nuts/bolt.
4. Remove the engine mount bracket.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the engine mount bracket and nuts.

Tighten

• | Tighten the engine mount bracket-to-hydro mount nut to 63 N·m (46 lb ft).

• | Tighten the engine mount bracket bolt to 51 N·m (38 lb ft).

• | Tighten the 2 engine mount bracket nuts to 51 N·m (38 lb ft).

2. Remove the J 28467-B .
3. Connect the negative battery cable.

## Engine Mount Replacement Left Side

#### Tools Required

J 28467-B , DW-117 (DW 110-060) Universal Engine Support Fixture

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

Notice: Refer to Engine Mounting Notice in the Preface section.

1. Disconnect the negative battery cable.

Notice: When raising or supporting the engine for any reason, do not use a jack under the oil pan, any sheet metal, or crankshaft balancer. Jacking against the oil pan may cause it to crack or break.

2. Support the engine assembly using the J 28467-B .
3. Remove the transaxle mount cage nut/bolts.
4. Remove the mount.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the engine mount (LH).

Tighten

• | Tighten the 4 transaxle mount cage-to-longitudinal member bolts to 63 N·m (46 lb ft).

• | Tighten the transaxle mount cage-to-transaxle mount bracket bolt to 63 N·m (46 lb ft).

• | Tighten the transaxle mount cage-to-transaxle mount bracket nut to 63 N·m (46 lb ft).

• | Tighten the transaxle mount cage through bolt to 110 N·m (81 lb ft).

2. Remove the J 28467-B .
3. Connect the negative battery cable.