For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Lock Pin Warning: Lock pin must be secured into the bench fixture to hold the transmission and prevent bodily injury. Tip Ensure the J 3289-20 is mounted to a bench that is properly supported and will support the weight of the transmission assembly without tipping. J-39890 adapter and an engine stand can be used as an alternative method for supporting the transmission assembly during repairs.

#### Special Tools

• | J 3289-20 Holding Fixture

• | J-39890 Transmission Holding Fixture Adapter

2 | J 21366 Torque Converter Holding Strap
3 | Torque Converter Assembly Tip Failure to raise the torque converter straight up could damage the torque converter clutch lip seal inside the torque converter clutch assembly.

#### Special Tool

J 46409 Torque Converter Lifting Handles