For 1990-2009 cars

1. Remove the transmission fluid baffle bolts/screws (807) and the transmission fluid baffle (803).
2. Remove the lube fluid pipe retainer bolt/screw (806).
3. Remove the lube fluid pipe retainer (805).
4. Remove the lube fluid pipe (804).
5. Inspect the torque converter housing for damage. If the bearings are faulty, the converter housing requires replacement.

Note: Do not bend or damage the lube fluid pipe (804).

6. Using a plastic hammer, install the lube fluid pipe (804).
7. Place the 4 chip collector magnets (808) onto the transmission fluid baffle (803).

Caution: Refer to Fastener Caution in the Preface section.

8. Install the transmission fluid baffle (803) and the 3 - M6 x 1.0 x 14 mm transmission fluid baffle bolts (807) and tighten to 5 N·m (44 lb in).
9. Install the lube fluid pipe retainer (805) and the M6 x 1.0 x 14 mm lube fluid pipe retainer bolt (806) into the torque converter housing assembly and tighten to 5 N·m (44 lb in).