For 1990-2009 cars

Checks | Actions
--- | ---
Check for mismatched or uneven tires. | Replace the tires.
Check for a broken or a sagging spring. | Replace the spring.
Check for a radial tire lateral force. |

• | Check the wheel alignment.

• | Switch the tire and the wheel assemblies.

• | Replace the tires, as needed.

Check the front wheel alignment. |

• | Align the front wheels.

• | Reseat the pinion valve assembly.

• | Replace the pinion valve assembly, as needed.

Check for front-brake dragging. | Adjust the front brakes.