For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: After cleaning the transmission components, allow to air dry. Do not use cloth or paper towels in order to dry any transmission components. Lint from the towels can cause component failure. Notice: Do not reuse cleaning solvents. Previously used solvents may deposit sediment which may damage the component.

#### Preliminary Procedures

1. Thoroughly clean the housing with clean solvent.
2. Inspect the piston bores and retainer ring grooves for wear, damage or porosity.

1 | 1-2-3-4 Clutch Spring Retainer Groove
2 | 1-2-3-4 Clutch Piston Bore
3 | Low and Reverse Clutch Spring Retainer Groove
4 | Low and Reverse Clutch Piston Bore
5 | Clutch Oil Passages
6 | Air Bleed Passages