For 1990-2009 cars

Table 1: | 1-2-3-4 Clutch Piston Installation
Table 2: | Low and Reverse Clutch Piston Installation

### 1-2-3-4 Clutch Piston Installation

Callout | Component Name
--- | ---
1 | 1-2-3-4 Clutch Piston Tip DT-47798 prevents the piston seal lip from damage during installation. Apply a thin coat of ATF to the I.D. of DT-47798 to ease the installation of the piston.

#### Special Tool

DT-47798 Seal Protector

2 | 1-2-3-4 Clutch Spring
3 | 1-2-3-4 Clutch Spring Retainer Tip

1. Place the retainer onto DT-47799-1 which is part of DT-47799 . Compressing the spring using DT-47799-2 which is part of DT-47799 , will install the retainer into the retainer groove.
2. Apply shop air to the clutch fluid feed hole in the clutch housing to verify proper piston operation.

#### Special Tool

DT-47799 Clutch Piston Spring Compressor

### Low and Reverse Clutch Piston Installation

Callout | Component Name
--- | ---
1 | Low and Reverse Clutch Piston Tip DT-47807 prevents the piston seal lip from damage during installation. Apply a thin coat of ATF to the I.D. of DT-47807 to ease the installation of the piston.

#### Special Tool

DT-47807 Clutch Piston Seal Protector

2 | Low and Reverse Clutch Spring
3 | Low and Reverse Clutch Spring Retainer

#### Procedure

1. Place the retainer onto DT-47794-1 which is part of DT-47794. Compressing the spring using DT-47794-2 which is part of DT-47794, will install the retainer into the retainer groove.
2. Apply shop air to the clutch fluid feed hole in the clutch housing to verify proper piston operation.

#### Special Tool

DT-47794 Spring Compressor