For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the electrical connector.
3. Remove the motor actuating rod by snapping it out of the lever with needle-nose pliers.
4. Remove the motor lever.
5. Remove the motor retaining bolts.
6. Remove the mode door motor.

### Installation Procedure

1. Install the mode door motor.
2. Install the motor retaining screws and tighten.
3. Install the motor lever by pressing it onto its shaft.
4. Install the actuating rod.
5. Connect the electrical connector.
6. Connect the negative battery cable.