For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the engine cover. Refer to Engine Cover Replacement.
3. Remove the charge air cooler outlet hose. Refer to Charge Air Cooler Inlet Pipe and Outlet Pipe Replacement.
4. Disconnect the removed electric throttle control (ETC) connector.
5. Remove the throttle body.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the throttle body using the body retaining bolts and nuts and tighten to 9 N·m (79.7 lb in).
2. Connect the ETC connector.
3. Install the charge air cooler outlet hose.
4. Install the engine cover. Refer to Engine Cover Replacement.
5. Connect the negative battery cable.