For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement.
2. Remove the bolt that secures the rear seat side bolster cushion.
3. Lift and remove the rear seat side bolster cushion.

### Installation Procedure

1. Slide the rear seat side bolster cushion into the retaining brackets.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the rear seat side bolster cushion with the bolt and tighten to 25 N·m (18 lb ft).
3. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement.