For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Remove the battery negative cable.
2. Remove the radiator grill upper cover.
3. Remove the radiator grill lower cover.
4. Disconnect the auxiliary cooling fan connector.
5. Remove the auxiliary cooling fan retaining bolts.
6. Remove the auxiliary cooling fan downward.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

Caution: To help avoid personal injury or damage to the vehicle, a bent, cracked, or damaged fan blade or housing should always be replaced.

1. Install the auxiliary cooling fan and the retaining bolts.

Tighten
Tighten the auxiliary cooling fan tightening bolts to 4 N·m (35 lb in).

2. Install the radiator grill upper and lower covers.
3. Connect the battery negative cable.