For 1990-2009 cars

### Removal Procedure

1. Remove the vacuum hose.
2. Remove the intake manifold tuning (IMT) valve solenoid. Refer to Intake Manifold Tuning Valve Actuator Solenoid Replacement.
3. Remove the IMT vacuum tank.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the IMT vacuum tank using the retaining bolts and tighten to 8 N·m (71 lb in).
2. Install the IMT solenoid. Refer to Intake Manifold Tuning Valve Actuator Solenoid Replacement.
3. Install the vacuum hose.