For 1990-2009 cars

Application | Ref No. | Quantity | Size | Specification
--- | --- | --- | --- | ---
Metric | English
A/Trans Fluid Pump Bolt to Converter Housing

- First Pass

200

8

M8x33

10 N·m

89 lb in

- Final Pass

200

8

M8x33

45 degrees

A/Trans Fluid Pump Cover Bolt | 302 | 23 | M6x25 | 12 N·m | 106 lb in
Control Solenoid Valve Assembly (w/TCM and Body) to Case Bolt | 4 | 12 | M6x97 | 12 N·m | 106 lb in
Control Solenoid Valve Assembly (w/TCM and Body) to Case Bolt | 6 | 3 | M5x40.5 | 8 N·m | 71 lb in
Control Valve Body Assembly (Complete) Bolt | 400 | 1 | M5x40.5 | 8 N·m | 71 lb in
Control Valve Body to Case Bolt | 9 | 2 | M6x53 | 12 N·m | 106 lb in
Control Valve Body to Case Bolt | 10 | 9 | M6x60 | 12 N·m | 106 lb in
Control Valve Body Cover Bolt | 1 | 13 | M6x30 | 12 N·m | 106 lb in
Drain Plug | 64 | 1 | 1/8"-27 NPTF | 12 N·m | 106 lb in
Fluid Level Hole Plug | 63 | 1 | 1/8"-27 NPTF | 12 N·m | 106 lb in
Fluid Pressure Test Hole Plug | 51 | 1 | 1/8"-27 NPTF | 12 N·m | 106 lb in
Front Differential Carrier Baffle Bolt - Converter Housing | 204 | 2 | M6x25 | 12 N·m | 106 lb in
Front Differential Carrier Baffle Bolt - Case | 61 | 2 | M6x16 | 12 N·m | 106 lb in
Input Shaft Support Bolt | 57 | 3 | M6x50 | 12 N·m | 106 lb in
Input Speed Sensor Bolt | 20 | 1 | M6x23 | 12 N·m | 106 lb in
Manual Shaft Detent Spring | 16 | 1 | M6x16 | 12 N·m | 106 lb in
Output Speed Sensor Bolt | 14 | 1 | M6x18 | 12 N·m | 106 lb in
Torque Converter and Differential Housing Bolt

- First Pass

26

15

M8x30

10 N·m

89 lb in

- Final Pass

26

15

M8x30

50 degrees

--

*Reference number refers to the component callout number in Disassembled Views