For 1990-2009 cars

### Removal Procedure

1. Remove the battery and tray.
2. Remove the air filter housing.
3. Remove the oil cooler pipe line bolts (1, 2) from the transaxle.
4. Remove the oil cooler pipe support bracket bolt (3).
5. Raise and suitably support the vehicle.
6. Place a drain pan or suitable container under the vehicle.
7. Disconnect the hoses from the radiator side.
8. Remove the oil cooler line assembly.

### Installation Procedure

1. Install the oil cooler line assembly to the transaxle.
2. Connect the hoses to the radiator side.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the oil cooler pipe support bracket bolt (3).

Tighten
Tighten the oil cooler pipe support bracket bolt to 10 N·m (89 lb in).

4. Install the oil cooler pipe line bolts (1, 2) to the transaxle.

Tighten
Tighten the oil cooler pipe line bolts to 20 N·m (15 lb ft).

5. Install the air filter housing.
6. Install the battery and tray.
7. Check the fluid level.