For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the oil filter.
3. Remove the oil filter adapter retaining bolts and oil filter adapter.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the oil filter adapter using the retaining bolts and tighten to 23 N·m (17 lb ft).
2. Install the oil filter and tighten to 14 N·m (124 lb in).