For 1990-2009 cars

### Removal Procedure

1. Remove the transaxle from the vehicle. Refer to Transmission Replacement.
2. Remove the concentric slave cylinder retaining bolts.
3. Disconnect the concentric slave cylinder pipe from the concentric slave cylinder.

Note: When removing the bushing, Make sure not to remove it with excessive force.

4. Remove the bushing from the concentric slave cylinder pipe in the transaxle housing.
5. Remove the concentric slave cylinder pipe.
6. Remove the O-ring and the concentric slave cylinder.

### Installation Procedure

1. Install the O-ring and concentric slave cylinder.

Caution: Refer to Fastener Caution in the Preface section.

2. After installing the pipe screw provisionally, tighten the concentric slave cylinder retaining bolts and tighten to 8-12 N·m (71-106 lb in).
3. Tighten the pipe screw to 16 N·m (12 lb ft).
4. Install the bushing onto the transaxle housing.
5. Connect the pipe with bushing.
6. Install the transaxle into the vehicle. Refer to Transmission Replacement.