For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the camshaft position (CMP) sensor connector.
3. Remove the CMP sensor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the CMP sensor.

Tighten
Tighten the CMP sensor retaining bolt 12 N·m (106 lb in).

2. Connect the CMP sensor connector.
3. Connect the negative battery cable.