For 1990-2009 cars

Checks | Actions
--- | ---
Check for a lack of lubrication of the ball joints and the tie rod ends. | Replace the ball joints and the outer tie rods.
Check for damaged suspension components. | Replace the damaged suspension components.
Check for worn control arm bushings or tie rod ends. | Replace the control arm bushings or the tie rods.
Check for a loose stabilizer shaft link. | Tighten the stabilizer shaft link.
Check for loose wheel nuts. | Tighten the wheel nuts.
Check for loose suspension bolts or nuts. | Tighten the suspension bolts or the nuts.
Check for worn strut dampeners or strut mountings. |

• | Replace the strut dampeners.

• | Tighten the strut mounting bolts.

Check for an improperly positioned strut spring. | Adjust the strut spring to the proper position.