For 1990-2009 cars

### Removal Procedure

1. Set the park brake and chock the wheels.
2. Remove the air cleaner inlet hose and snorkel.
3. Disconnect the shift control cable from the range selector lever.
4. Remove the selector lever nut and lever.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the lever and selector lever nut and tighten to 15 N·m (11 lb ft).
2. Connect the shift control cable to the range selector lever.
3. Install the air cleaner inlet hose and snorkel.