For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Fluid Reservoir Bolts | 7.5 N·m | 66 lb in
Hydraulic Cylinder Pipe Fittings | 13 N·m | 10 lb ft
Intermediate Shaft-to-Steering Gear Pinion Pinch Bolt | 25 N·m | 18 lb ft
Outer Tie Rod Adjusting Nuts | 64 N·m | 47 lb ft
Outer Tie Rod Ball Joint Stud Nuts | 50 N·m | 37 lb ft
Power Steering Pump Bolts | 25 N·m | 18 lb ft
Power Steering Pump Pressure Pipe Fitting | 28 N·m | 21 lb ft
Pressure Pipe Bracket-to-Generator Bolt | 10 N·m | 7 lb ft
Pressure Pipe-to-Heat Shield Nut | 9 N·m | 80 lb in
Pressure Pipe-to-Steering Gear Inlet Fitting | 28 N·m | 21 lb ft
Return Pipe Bracket Bolts Near the Power Steering Pump | 14 N·m | 10 lb ft
Return Pipe Bracket Bolts Near the Radiator | 14 N·m | 10 lb ft
Return Pipe Bracket-to-Crossmember Bolts | 9 N·m | 80 lb in
Return Pipe-to-Steering Gear Outlet Fitting | 28 N·m | 21 lb ft
Steering Gear Mounting Bracket Nuts and Bolts | 60 N·m | 44 lb ft
Surge Tank Nuts | 5 N·m | 44 lb in