For 1990-2009 cars

## Maintenance Schedule Europe

Table 1: | Engine
Table 2: | Chassis and Body

#### Engine

Maintenance Item | Maintenance Interval
--- | ---
Kilometers or time in months, whichever comes first
x 1 000 km | 15 | 30 | 45 | 60 | 75 | 90 | 105 | 120
x 1,000 miles | 10 | 20 | 30 | 40 | 50 | 60 | 70 | 80
Months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96
Drive Belts (Alternator, Power Steering and A/C Belt)
2.0L/2.5L | I | I | I | I | I | I | I | I
2.0L Diesel | -- | I | -- | I | -- | I | -- | I
Engine Oil and Engine Oil Filter (1) (3)
2.0L/2.5L | R | R | R | R | R | R | R | R
2.0L Diesel | Replace every 30 000 km (20,000 mi) or 1 year
Cooling System Hose and Connections | I | I | I | I | I | I | I | I
Engine Coolant - DEX-COOL® (3) | See the remark (4) below.
Engine Coolant - Silicate based | I | I | R | I | I | R | I | I
Fuel Filter
2.0L | -- | -- | R | -- | -- | R | -- | --
2.0L Diesel | -- | -- | -- | R | -- | -- | -- | R
Fuel Filter (Integrated in Fuel Pump) - 2.5L | -- | -- | I | -- | -- | I | -- | --
Fuel Line and Connections | I | I | I | I | I | I | I | I
Air Cleaner Element (2) | I | I | R | I | I | R | I | I
Spark Plugs (5) 2.0L/2.5L | -- | I | -- | I | -- | I | -- | I
EVAP Canister, Vapor Lines and Solenoid Valve Filter | -- | -- | I | -- | -- | I | -- | --
PCV System | -- | I | -- | I | -- | I | -- | I
Timing Belt or Chain
2.0L/2.5L | Replace every 300 000 km
2.0L Diesel | See the remark (6) below.

#### Table Symbols:

I--Inspect these items and their related parts. If necessary, correct, clean, replenish, adjust or replace.

R--Replace or change.

#### Remarks:

(1) Change engine oil and the filter every 7 500 km (5,000 mi) or 6 months, whichever comes first, if the vehicle is operated under any of the following severe conditions:

• | Repeated short-distance driving less than 10 km (5 mi).

• | Extensive idling.

• | Driving on dusty roads.

(2) Inspect the air cleaner element every 7 500 km (5,000 mi) or 6 months if the vehicle is driven on dusty roads. If necessary, correct, clean, or replace.

(3) Refer to Fluid and Lubricant Recommendations .

(4) Inspect the engine coolant every 1 year or 15 000 km (10,000 mi) and replace it every 5 years or 240 000 km (150,000 mi).

(5) Replace every 160 000 km (100,000 mi).

(6) Inspect every 30 000 km (20,000 mi) or 2 years and replace every 160 000 km.

If the vehicle is mainly driven under the following severe conditions, replace every 60 000 km (36,000 mi):

• | Repeated short-distance driving less than 10 km (5 mi).

• | Extensive idling and/or slow-speed driving in stop-and-go traffic.

• | Driving on dusty roads.

• | Driving on hilly or mountainous terrain.

• | Towing a trailer.

• | Driving in heavy city traffic where the outside temperature regularly reaches 32°C (90°F) or higher.

• | Driving as a taxi, police, or delivery vehicle.

• | Frequent driving when outside temperature remains below freezing.

#### Chassis and Body

Maintenance Item | Maintenance Interval
--- | ---
Kilometers or time in months, whichever comes first
x 1 000 km | 15 | 30 | 45 | 60 | 75 | 90 | 105 | 120
x 1,000 miles | 9 | 18 | 27 | 36 | 45 | 54 | 63 | 72
Months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96
Air Filter (A/C) (4) | R | R | R | R | R | R | R | R
Exhaust Pipes and Mountings | I | I | I | I | I | I | I | I
Brake/Clutch Fluid (3) (5) | I | R | I | R | I | R | I | R
Front Brake Pads and Discs (6) | I | I | I | I | I | I | I | I
Rear Brake Pads Discs or Drums and Linings (6) | I | I | I | I | I | I | I | I
Parking Brake | I | I | I | I | I | I | I | I
Brake Line and Connections (Including Booster) | I | I | I | I | I | I | I | I
Manual Transaxle Oil (3) | I | I | I | I | I | I | I | I
Automatic Transaxle Fluid | See the remark (9) below.
The Condition and Inflation Pressure | See the remark (7) below.
Wheel Alignment (8) | Inspect when abnormal condition is noted.
Steering Wheel and Linkage | I | I | I | I | I | I | I | I
Power Steering Fluid and Lines (3) | I | I | I | I | I | I | I | I
Drive Shaft Boots | I | I | I | I | I | I | I | I
Safety Belts, Buckles and Anchors | I | I | I | I | I | I | I | I
Lubricate Locks, Hinges and Hood Latch | I | I | I | I | I | I | I | I

#### Table Symbols:

I--Inspect and if necessary correct, clean, replenish, or adjust.

R--Replace or change.

#### Remarks:

(3) Refer to Fluid and Lubricant Recommendations .

(4) More frequent maintenance is required if the vehicle is mainly driven on dusty roads.

(5) Change the brake/clutch fluid every 15 000 km (10,000 mi) if the vehicle is frequently driven under the following severe conditions:

• | Driving in hilly or mountainous terrain.

• | Towing a trailer.

(6) More frequent maintenance is required if the vehicle is mainly driven under the following severe conditions:

• | Repeated short-distance driving less than 10 km (5 mi).

• | Extensive idling and/or slow-speed driving in stop-and-go traffic.

• | Driving on dusty roads.

(7) Tire condition should be inspected before driving and tire pressure should be checked each time you fill your fuel tank or at least once a month using a tire pressure gage.

(8) If necessary, rotate and balance wheels.

(9) If equipped with the 5-speed Aisin 55-51LE automatic transaxle, a fluid change is not required. Also, routine inspection of the fluid is not required. Transaxle fluid inspection is only required if there is a symptom indicating a concern with the fluid.

If equipped with the 6-speed GF-6 6T40/45 automatic transaxle, inspect the fluid every 40 000 km (25,000 mi) and change the fluid every 160 000 km (100,000 mi). If the vehicle is mainly driven under the following severe conditions, change the fluid every 80 000 km (50,000 mi):

• | Driving in heavy city traffic where the outside temperature regularly reaches 32°C (90°F) or higher.

• | Driving on hilly or mountainous terrain.

• | Towing a trailer.

• | Driving as a taxi, police, or delivery vehicle.

## Maintenance Schedule Holden

Table 1: | Engine
Table 2: | Chassis and Body

#### Engine

Maintenance Item | Maintenance Interval
--- | ---
Kilometers or time in months, whichever comes first
x 1 000 km | 15 | 30 | 45 | 60 | 75 | 90 | 105 | 120
x 1,000 miles | 10 | 20 | 30 | 40 | 50 | 60 | 70 | 80
Months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96
Drive Belts (Alternator, Power Steering and A/C Belt) | Inspect every 10 000 km (6,000 mi).
Engine Oil and Engine Oil Filter (1) (3) | R | R | R | R | R | R | R | R
Cooling System Hose and Connections | I | I | I | I | I | I | I | I
Engine Coolant - DEX-COOL® (3) | See the remark (4) below.
Engine Coolant - Silicate Based | I | I | R | I | I | R | I | I
Fuel Filter (Integrated in Fuel Pump) (5) | -- | -- | I | -- | -- | I | -- | --
Fuel Line and Connections | I | I | I | I | I | I | I | I
Air Cleaner Element (2) | I | I | R | I | I | R | I | I
Spark Plugs | I | R | I | R | I | R | I | R
Spark Plug Wires | Inspect every 40 000 km (25,000 mi). Replace every 160 000 km (100,000 mi).
Evaporative Emission Canister and Vapor Lines | -- | -- | I | -- | -- | I | -- | --
PCV System | -- | I | -- | I | -- | I | -- | I
Timing Belt or Chain | Replace every 300 000 km (180,000 mi).

#### Table Symbols:

I--Inspect these items and their related parts. If necessary, correct, clean, replenish, adjust or replace.

R--Replace or change.

#### Remarks:

(1) Change engine oil and the filter every 7 500 km (5,000 mi) or 6 months, whichever comes first, if the vehicle is operated under any of the following severe conditions:

• | Repeated short-distance driving less than 10 km (5 mi).

• | Extensive idling.

• | Driving on dusty roads.

(2) Inspect the air cleaner element every 7 500 km (5,000 mi) or 6 months if the vehicle is driven on dusty roads. If necessary, correct, clean, or replace.

(3) Refer to Fluid and Lubricant Recommendations.

(4) Inspect the engine coolant every 12 months or 15 000 km (10,000 mi) and replace it every 5 years or 240 000 km (150,000 mi).

(5) Replace every 144 000 km (90,000 mi).

#### Chassis and Body

Maintenance Item | Maintenance Interval
--- | ---
Kilometers or time in months, whichever comes first
x 1 000 km | 15 | 30 | 45 | 60 | 75 | 90 | 105 | 120
x 1,000 miles | 9 | 18 | 27 | 36 | 45 | 54 | 63 | 72
Months | 12 | 24 | 36 | 48 | 60 | 72 | 84 | 96
Interior Air Filter (A/C) (8) | R | R | R | R | R | R | R | R
Exhaust Pipes and Mountings | I | I | I | I | I | I | I | I
Brake/Clutch Fluid (3) (4) | I | R | I | R | I | R | I | R
Rear Brake Drums and Linings (5) | I | I | I | I | I | I | I | I
Front Brake Pads and Discs (5) | I | I | I | I | I | I | I | I
Park Brake | I | I | I | I | I | I | I | I
Brake Line and Connections (Including Booster) | I | I | I | I | I | I | I | I
Chassis and Underbody Bolts and Nuts Tight/Secure | I | I | I | I | I | I | I | I
Automatic Transaxle Fluid | See the remark (9) below.
Wheel Alignment (6) | Inspect when abnormal condition is noted.
The Condition and Inflation Pressure | See the remark (7) below.
Steering Wheel and Linkage | I | I | I | I | I | I | I | I
Power Steering Fluid and Lines (3) | I | I | I | I | I | I | I | I
Drive Shaft Boots | I | I | I | I | I | I | I | I
Seat Belts, Buckles and Anchors | I | I | I | I | I | I | I | I
Lubricate Locks, Hinges and Hood Latch | I | I | I | I | I | I | I | I

#### Table Symbols:

I--Inspect and if necessary correct, clean, replenish, or adjust.

R--Replace or change.

#### Remarks:

(3) Refer to Fluid and Lubricant Recommendations.

(4) Change the brake/clutch fluid every 15 000 km (10,000 mi) if the vehicle is frequently driven under the following severe conditions:

• | Driving in hilly or mountainous terrain.

• | Towing a trailer or a caravan.

(5) More frequent maintenance is required if the vehicle is mainly driven under the following severe conditions:

• | Repeated short-distance driving less than 10 km (5 mi).

• | Extensive idling and/or slow-speed driving in stop-and-go traffic.

• | Driving on dusty roads.

(6) If necessary, rotate and balance the wheels.

(7) Tire condition should be inspected before driving and tire pressure should be checked each time you fill your fuel tank or at least once a month using a tire pressure gage.

(8) More frequent maintenance is required if the vehicle is mainly driven on dusty roads.

(9) If equipped with the 5-speed Aisin 55-51LE automatic transaxle, a fluid change is not required. Also, routine inspection of the fluid is not required. Transaxle fluid inspection is only required if there is a symptom indicating a concern with the fluid.

If equipped with the 6-speed GF-6 6T40/45 automatic transaxle, inspect the fluid every 40 000 km (25,000 mi) and change the fluid every 160 000 km (100,000 mi). If the vehicle is driven under the following severe conditions, change the fluid every 80 000 km (50,000 mi):

• | Driving in heavy city traffic where the outside temperature regularly reaches 32°C (90°F) or higher.

• | Driving on hilly or mountainous terrain.

• | Towing a trailer.

• | Driving as a taxi, police, or delivery vehicle.

## Maintenance Schedule Except Europe, Holden

Table 1: | Engine
Table 2: | Chassis and Body

#### Engine

Maintenance Item | Maintenance Interval
--- | ---
Kilometers or time in months, whichever comes first
x 1 000 km | 10 | 20 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100
x 1,000 miles | 6 | 12 | 18 | 24 | 30 | 36 | 42 | 48 | 54 | 60
Months | 6 | 12 | 18 | 24 | 30 | 36 | 42 | 48 | 54 | 60
Drive Belts (Alternator, Power Steering and A/C Compressor) | I | I | I | I | I | I | I | I | I | I
Engine Oil & Engine Oil Filter (1) (3) | Replace every 15 000 km (9,400 mi)
Cooling System Hose and Connections | I | I | I | I | I | I | I | I | I | I
Engine Coolant-DEX-COOL® (3) | See the remark (4) below.
Engine Coolant - Silicate Based | I | I | I | R | I | I | I | R | I | I
Fuel Filter | 2.0L | -- | -- | -- | R | -- | -- | -- | R | -- | --
Fuel Filter (Integrated in Full Pump) | 2.5L | -- | -- | -- | -- | I | -- | -- | -- | -- | I
Fuel Line and Connections | I | I | I | I | I | I | I | I | I | I
Air Cleaner Element (2) | I | I | I | R | I | I | I | R | I | I
Spark Plugs | 2.0L/2.5L | Inspect every 40 000 km (25,000 mi) Replace every 160 000 km (100,000 mi)
2.0L/2.5L Leaded Fuel | -- | I | -- | I | -- | R | -- | I | -- | I
EVAP Canister, Vapor Lines and Solenoid Valve Filter | -- | -- | -- | I | -- | -- | -- | I | -- | --
Timing Belt or Chain | Replace every 300 000 km (180,000 mi)
PCV System | -- | -- | I | -- | -- | -- | -- | -- | I | --

#### Table Symbols:

I - Inspect these items and their related parts. If necessary, correct, clean, replenish, adjust or replace.

R - Replace or change.

#### Remarks:

(1) Change engine oil and the filter every 5 000 km (3,000 mi) or 3 months, whichever comes first, if the vehicle is operated under any of the following severe conditions:

• | Repeated short-distance driving less than 10 km (5 mi).

• | Extensive idling.

• | Driving on dusty roads.

(2) Inspect the air cleaner element every 5 000 km (3,000 mi) or 3 months if the vehicle is driven on dusty roads. If necessary, correct, clean, or replace.

(3) Refer to Fluid and Lubricant Recommendations.

(4) Inspect the engine coolant every 6 months or 10 000 km (6,000 mi) and replace it every 5 years or 240 000 km (150,000 mi).

#### Chassis and Body

Maintenance Item | Maintenance Interval
--- | ---
Kilometers or time in months, whichever comes first
x 1 000 km | 10 | 20 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100
x 1,000 miles | 6 | 12 | 18 | 24 | 30 | 36 | 42 | 48 | 54 | 60
Months | 6 | 12 | 18 | 24 | 30 | 36 | 42 | 48 | 54 | 60
Interior Air Filter (A/C) (4) | R | R | R | R | R | R | R | R | R | R
Exhaust Pipes and Mountings | I | I | I | I | I | I | I | I | I | I
Brake/Clutch Fluid (3) (5) | I | I | R | I | I | R | I | I | R | I
Front Brake Pads and Discs (6) | I | I | I | I | I | I | I | I | I | I
Rear Brake Pads Discs or Drums and Linings (6) | I | I | I | I | I | I | I | I | I | I
Park Brake | I | I | I | I | I | I | I | I | I | I
Brake Line and Connections (Including Booster) | I | I | I | I | I | I | I | I | I | I
Manual Transaxle Oil (3) | I | I | I | I | I | I | I | I | I | I
Chassis and Underbody Bolts and Nuts Tight/Secure | I | I | I | I | I | I | I | I | I | I
Automatic Transaxle Fluid | See the remark (9) below
Tire Condition and Inflation Pressure | See the remark (7) below
Wheel Alignment (8) | Inspect when abnormal condition is noted
Steering Wheel and Linkage | I | I | I | I | I | I | I | I | I | I
Power Steering Fluid and Lines (3) | I | I | I | I | I | I | I | I | I | I
Drive Shaft Boots | I | I | I | I | I | I | I | I | I | I
Seat Belts, Buckles and Anchors | I | I | I | I | I | I | I | I | I | I
Lubricate Locks, Hinges and Hood Latch | I | I | I | I | I | I | I | I | I | I

#### Table Symbols:

I - Inspect and if necessary correct, clean , replenish, or adjust.

R - Replace or change.

#### Remarks:

(3) Refer to Fluid and Lubricant Recommendations.

(4) More frequent maintenance is required if the vehicle is mainly driven on dusty roads.

(5) Change the brake/clutch fluid every 15 000 km (9,000 mi) if the vehicle is frequently driven under the following severe conditions:

• | Driving in hilly or mountainous terrain.

• | Towing a trailer.

(6) More frequent maintenance is required if the vehicle is mainly driven under the following severe conditions:

• | Repeated short-distance driving less than 10 km (5 mi).

• | Extensive idling and/or slow-speed driving in stop-and-go traffic.

• | Driving on dusty roads.

(7) Tire condition should be inspected before driving and tire pressure should be checked each time you fill your fuel tank or at least once a month using a tire pressure gage.

(8) If necessary, rotate and balance the wheels.

(9) If equipped with the 5-speed Aisin 55-51LE automatic transaxle, a fluid change is not required. Also, routine inspection of the fluid is not required. Transaxle fluid inspection is only required if there is a symptom indicating a concern with the fluid.

If equipped with the 6-speed GF-6 6T40/45 automatic transaxle, inspect the fluid every 40 000 km (25,000 mi) and change the fluid every 160 000 km (100,000 mi). If the vehicle is driven under the following severe conditions, change the fluid every 80 000 km (50,000 mi):

• | Driving in heavy city traffic where the outside temperature regularly reaches 32°C (90°F) or higher.

• | Driving on hilly or mountainous terrain.

• | Towing a trailer.

• | Driving as a taxi, police, or delivery vehicle.