For 1990-2009 cars

Checks | Causes
--- | ---
Fluid Pump Assembly (201) |

• | Inspect for loose Fluid Pump Bolts (204)

• | Inspect for leaking or damaged Fluid Pump Outlet Seals (24) and Oil Filter Seal

• | Inspect for improperly installed, restricted or damaged Oil Filter (203)

• | Inspect for sticking Line Pressure Blow Off Valve (304)

• | Inspect for worn, sticking or damaged Pressure Regulator Valve (309) or Pressure Regulator Valve Spring (308)

• | Inspect for damaged or restricted oil ports in the Oil Pump Body (303)

Torque Converter Housing (208) |

• | Inspect for missing or restricted Differential Lube Oil Circuit Orifice

• | Inspect for missing Front differential Carrier Baffle (205)

Control Solenoid Valve Assembly (w/Body and TCM) (7) | Inspect for leaking or damaged Filter Plate Assembly Seals (8)
Case Assembly (50) |

• | Inspect for proper fluid level

• | Inspect for missing Lube Oil Circuit Orifice or Front Differential Carrier Baffle (62)

• | Inspect for leaking or damaged Valve Body Spacer Plate Assembly (12)

• | Inspect for damaged or leaking Fluid Check Valve (55)

• | Inspect for leaking, damaged or broken Fluid Level Control Valve (13)

Torque Converter Assembly (28) |

• | Inspect for damaged Torque Converter Clutch Seal (inside converter assembly)

• | Inspect for damaged or disengaged Torque Converter hub to Oil Pump Drive Gear