For 1990-2009 cars

### Removal Procedure

1. Remove the bolt of impact beam-to-radiator centermember.
2. Remove the bolts of impact beam-to-front suspension centermember.
3. Remove the impact beam.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

Install the impact beam with bolts-to-radiator centermember and front suspension centermember.

Tighten
Tighten the bolts-to-radiator centermember and front suspension centermember to 100 N·m (74 lb ft).