For 1990-2009 cars

### Removal Procedure

1. Remove the door seal trim. Refer to Door Bottom Auxiliary Sealing Strip Replacement.
2. Remove the bolts on the door and on the body.
3. Remove the door hold-open link.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the door hold-open link to the door and the body with the bolts.

• | Tighten the door hold-open link-to-body bolt to 25 N·m (18 lb ft).

• | Tighten the door hold-open link-to-door bolts to 9 N·m (80 lb in).

2. Install the door seal trim. Refer to Door Bottom Auxiliary Sealing Strip Replacement.